For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .

1 | Front Side Door Lock Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tip Disconnect the lock cylinder and outside handle rod from the lock assembly. Tighten
10 N·m (89 lb in)

2 | Front Side Door Lock Assembly

#### Procedure

1. Release the door lock cable retainers from the door.
2. Disconnect the door lock electrical connector.