For 1990-2009 cars

### Removal Procedure

1. Disconnect the engine wiring harness electrical connector (4) from the exhaust camshaft position (CMP) sensor.
2. Remove the CMP sensor bolt. (Intake CMP shown, exhaust CMP similar)
3. Remove the CMP sensor.

### Installation Procedure

Important: Inspect the CMP sensor for damage. Replace as necessary.

1. Lubricate the CMP sensor O-ring seal with clean engine oil.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor. (Intake CMP shown, exhaust CMP similar)
3. Install the CMP sensor bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Connect the engine wiring harness electrical connector (4) to the exhaust CMP sensor.