For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Stabilizer Shaft Insulator Mounting Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tip

• | The mounting bolts DO NOT have to be removed to perform this procedure. Loosen the bolts until the bracket is loose enough to slide the insulator along the stabilizer shaft.

• | Support the lower control arm with a jack stand in order to ease the removal and installation of the link.

Tighten
55 N·m (41 lb ft)

2 | Stabilizer Shaft Bracket
3 | Stabilizer Shaft Insulator Tip Before removing the insulator, clean the area around the insulator and apply a small amount of silicone spray.