For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Recover the A/C refrigerant. Refer to Refrigerant Recovery and Recharging .

1 | A/C Compressor Tube Assembly Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 16 N·m (12 lb ft)
2 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

3 | Thermal Expansion Valve Bolt Tighten 16 N·m (12 lb ft)
4 | Sealing Washer

#### Procedure

Remove and discard sealing washer. Refer to Sealing Washer Replacement .

5 | Thermal Expansion Valve