For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement .
2. Program the remote control door lock receiver after replacement. Refer to Control Module References .

1 | Remote Control Door Lock Transmitter Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Push the 2 tabs toward the module assembly in order to release the module from the panel.