For 1990-2009 cars

#### Special Tools

J 43653 Flywheel Holding Tool

1. Ensure that J 43653 flywheel holding tool is installed and engaging the flywheel to prevent crankshaft rotation.
2. Remove the flywheel attaching bolts.
3. Remove the flywheel, if the vehicle has a manual transmission.
4. Remove the pilot bearing. Refer to Clutch Pilot Bearing Replacement for manual transmission.
5. Remove J 43653 flywheel holding tool .