For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left rear wheel. Refer to Tire and Wheel Removal and Installation .
2. Remove the left rear wheelhouse liner. Refer to Rear Wheelhouse Panel Liner Replacement .
3. Remove the pressure relief valve. Refer to Pressure Relief Valve Replacement .
4. Reach into the rear compartment through the opening and locate the child safety release cable and pull handle to unlatch deck lid.

1 | Rear Compartment Tip The handle will be on the inside of carpet. The cable runs between the rear wheelhouse and carpet. Pull the handle through the slot in the carpet.