For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the door sill trim. Refer to Door Sill Plate Replacement.
2. Remove the lock pillar trim panel. Refer to Body Lock Pillar Trim Panel Replacement
3. Remove the floor console trim plate. Refer to Front Floor Console Replacement.

1 | Rear Window Panel Trim Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Open the rear stowage compartment to access nuts.

Tighten
2 N·m (18 lb in)

2 | Rear Window Panel Trim Assembly
3 | Rear Window Panel Trim Retainer (Qty: 13)