For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Remove the power seat switch. Refer to Power Seat Switch Replacement.
3. Remove the front seat cushion cover and pad. Refer to Seat Cushion Trim Cover and Pad Replacement .
4. Remove the front seat belt buckle. Refer to Front Seat Belt Buckle Replacement.

1 | Seat Back Cushion Frame Retainer Clip (Qty: 2)
2 | Driver Seat Cushion Frame with Adjuster

#### Procedure

1. Spread the seat back frame pivot brackets apart enough to remove the seat back assembly from the seat cushion frame.
2. If working on the passenger seat, re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References.