For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the top from the vehicle. Refer to Folding Top Replacement .

1 | Outboard Spring Rivet

#### Procedure

Drill out the rivet to remove the springs.

2 | Outboard Spring

#### Procedure

1. Spring has minimal tension when top is in stowed position.
2. Remove the spacer.

3 | Inboard Spring Tip

• | Inboard spring has minimal tension when top is in raised position.

• | Inboard spring is larger in diameter than outboard spring.

• | Inboard/Outboard springs have opposite winding.