For 1990-2009 cars

# Door Glass Comes in Contact with Convertible Top (Adjust Number 4 Bow)

Subject: | Door Glass Comes in Contact with Convertible Top (Adjust Number 4 Bow)

Models: | 2006-2009 Pontiac Solstice

| 2007-2009 Saturn SKY

| 2007-2009 Opel GT

| 2007-2009 Daewoo G2X

This bulletin is being revised to add model years. Please discard Corporate Bulletin Number 07-08-67-005A (Section 08 - Body and Accessories).

### Condition

Some customers may comment that the door glass is coming in contact with the webbing of the convertible top in the upper rear corners.

### Cause

This condition may be caused by the number 4 bow being out of adjustment.

### Correction

1. If the glass looks good to the opening with no windnoise or water leaks complaints, then proceed with the number 4 bow adjustment. If the door glass is out of alignment, align or adjust the glass.
2. Use a 10 mm open end wrench to loosen the jam nut. Move the upstop counterclockwise to tighten top cover. Each turn moves the upstop 1 mm (.039 in). There is a 4-to-1 ratio between the upstop and the top of the bow (one turn moves the #4 bow 4 mm (.16 in) at the top). Two turns of the upstop should be sufficient to tighten a loose top. Refer to the illustration above.

### Warranty Information

Fro vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C9807* | Adjust Upstop | 0.2 hr
* This is a unique labor operation for bulletin use only. It will not be published in the Labor Time Guide.