For 1990-2009 cars

This is intended to provide general guidelines for urethane adhesive bonding of full panel replacement in regards to collision repair procedures.

Sectioning, partial panel of full panels, is not supported by General Motors unless specifically documented in a Service Bulletin or Manual.

Important:

• | Prepare the surfaces to be bonded according to the adhesive manufacturer's recommendations. Many adhesive manufacturers have different preparation methods. Do not intermix adhesive manufacturers systems. Mixing materials from different manufacturers can produce unsatisfactory results.

• | DO NOT top coat any adhesive bonding mating surface. Use primer only on bonding surfaces. Refer to adhesive manufacturer's recommendations for priming applications.

Adhesives currently meeting the performance requirements include products manufactured by 3M and Dow Automotive. At this time, ONLY the adhesive products listed below meet this guideline:

3M | Dow 1-800-453-3779
--- | ---
3M Fast Cure Windshield Urethane HV, PN 08690 (one part and requires 3M Single Step Primer, PN 08681 | U-400HV (one part and requires associated primers)