For 1990-2009 cars

1. Remove the oil receiver.
2. Remove the oil trough bolt.
3. Remove the oil trough.
4. Using a suitable prying tool, remove the output shaft seal from the extension housing.
5. Remove the reverse control lever restrictor pin plug. Discard the plug. A new plug is required for assembly.
6. Remove the roll pin for the reverse control lever restrictor.
7. Remove the reverse control lever restrictor.