For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
3. Remove the drive belt. Refer to Drive Belt Replacement .

1 | Engine Harness Generator Connector
2 | Engine Harness Ground Terminal Boot
3 | Engine Harness Ground Terminal Nut Notice: Refer to Fastener Notice in the Preface section. Tighten 20 N·m (15 lb ft)
4 | Engine Harness Ground Terminal
5 | Generator Bolt (Qty: 3) Tighten 22 N·m (16 lb ft)
6 | Generator