For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front hinge pillar molding. Refer to Body Hinge Pillar Trim Panel Replacement.

1 | Driver Foot Rest Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Remove the push-on rubber covers to access the nuts.

Tighten
6 N·m (53 lb in)

2 | Driver Foot Rest Assembly
3 | Driver Foot Rest Stud (Qty: 2)