For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the side front weatherstrip. Refer to Folding Top Side Front Weatherstrip Replacement.

1 | Folding Top Side Front Weatherstrip Retainer Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Folding Top Side Front Weatherstrip Retainer Tip

• | If necessary, adjust the weatherstrip retainer. Refer to Folding Top Side Front Weatherstrip Retainer and Side Rear Weatherstrip Retainer Adjustment.

• | Inspect the fit of the seal to door glass.

• | Cycle the top and inspect the joint between side front/rear rail weatherstrips.