For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement.
2. Remove the right rear wheelhouse panel. Refer to Rear Wheelhouse Panel Liner Replacement.

1 | Radio Antenna Assembly
2 | Radio Antenna Base Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
3 | Radio Antenna Bracket Stud Cap
4 | Radio Antenna Bolt Tighten 9 N·m (80 lb in)
5 | Radio Antenna Bracket Assembly