For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the hood in order to access the front marker lamp screw.

1 | Front Side Marker Lamp Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Side Marker Lamp Assembly

#### Procedure

1. Remove the screw.
2. Disconnect the electrical connector from the forward lamp harness.
3. Slightly lift the retention clip upward on the lamp assembly.
4. Slide the lamp forward from under the bracket assembly.
5. Remove the lamp and electrical harness as one assembly.