For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the LF wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
2. Drain the washer solvent into a suitable container.
3. Disconnect the washer pump electrical connector.
4. Disconnect the washer hose from the washer pump spout.

1 | Washer Pump Kit with Seal Tip Use a flat-bladed tool in order to pry the washer pump from the washer container.
2 | Washer Pump Seal Tip Discard the old washer pump seal.