For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides and overview of each diagnostic category.

### DTC Descriptor

DTC 2036: Internal Electronic Performance 2

### Circuit/System Description

The passenger presence system (PPS) is used to monitor the pressure profile of any occupant that is sitting in the front outboard passenger seat and communicates the profile classification to the sensing and diagnostic module (SDM). The SDM will either enable or suppress the deployment of the instrument panel (I/P) module based on the profile classification of the occupant. If the PPS detects DTC 2036 within itself, the PPS will communicate to the SDM through a dedicated serial data circuit that a PPS fault is present. The SDM will set DTC B0081 indicating a problem within the PPS and suppress the deployment of the I/P module and illuminate the AIR BAG indicator.

### Conditions for Running the DTC

Ignition voltage is between 9-16 volts

### Conditions for Setting the DTC

The PPS has detected an internal fault.

### Action Taken When the DTC Sets

• | The PPS will set a DTC and then communicate with the SDM.

• | The SDM will set DTC B0081.

• | The SDM disables the I/P module deployment loop.

• | The PPS will illuminate the passenger air bag status OFF indicator.

• | The SDM requests the instrument panel cluster (IPC) to illuminate the AIR BAG indicator.

### Conditions for Clearing the DTC

• | The condition for setting the DTC no longer exists.

• | A history DTC will clear once 100 malfunction-free ignition cycles have occurred.

### Reference Information

#### Schematic Reference

SIR Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

SIR System Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

Important: When removing connectors inspect for damage or corrosion. Damage or corrosion in the following requires repair or replacement of the affected.

• | PPS module

• | PPS module wiring harness

Verify that DTC 2036 is not set.

⇒ | If the DTC is set, replace the PPS module.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Control Module References for PPS module replacement, setup, and programming