For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the charge air cooler outlet pipe. Refer to Charge Air Cooler Outlet Pipe Replacement .
3. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement .
4. Remove the generator. Refer to Generator Replacement .

1 | A/C Compressor and Condenser Hose Assembly Nut Notice: Refer to Fastener Notice in the Preface section. Tip A/C compressor hose to A/C evaporator hose Tighten
9 N·m (80 lb in)

2 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement .

3 | A/C Compressor and Condenser Hose Assembly Nut Tip A/C compressor hose to A/C condenser Tighten 9 N·m (80 lb in)
4 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement .

5 | A/C Compressor and Condenser Hose Assembly Bolt Tighten 22 N·m (16 lb ft)
6 | Sealing Washer

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement .

7 | A/C Compressor and Condenser Hose Assembly