For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC P0563 : System Voltage High

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
IGN | P0562 | P0562 | -- | --
Ground | -- | P0562 | -- | --

### Circuit/System Description

The engine control module (ECM) monitors the system voltage to ensure that the voltage stays within the proper range. Damage to components, and incorrect data may occur when the voltage is out of range.

### Conditions for Running the DTC

• | The vehicle speed is above 8 km/h (5 mph).

• | The system voltage is between 9.5-18 volts.

### Conditions for Setting the DTC

The ECM detects a system voltage above 16 volts for less than 1 second.

### Action Taken When the DTC Sets

The instrument panel cluster (IPC) illuminates the charge indicator.

### Conditions for Clearing the DTC

DTC P0563 is a C type DTC.

### Diagnostic Aids

• | A possible cause of this DTC could be overcharging with a battery charger or jump starting.

• | A high voltage value in multiple modules indicates a concern in the charging system.

### Reference Information

#### Schematic Reference

Engine Controls Schematics for the 2.0L engine.

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Charging System Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. Engine running measure and record the voltage at the battery terminals. Verify that the battery voltage is 12.6-15.5 volts

⇒ | If the battery voltage is not within the specified range, refer to Charging System Test

2. Engine running, observe the scan tool ECM Ignition 1 signal parameter. The voltage should be between 12.5 and 15.5 volts.

⇒ | If greater than specified value , replace the ECM.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Control Module References for ECM replacement, setup, and programming.