For 1990-2009 cars

1. If removed, install the reverse control lever restrictor.
2. Install a new reverse control lever restrictor roll pin.

Caution: Refer to Fastener Caution in the Preface section.

3. Install a new reverse restrictor pin plug. Tighten the reverse restrictor pin plug to 19 N·m (14 lb ft).
4. Install the oil receiver.
5. Install the oil trough.
6. Install the oil trough bolt. Tighten the oil trough bolt to 11 N·m (97 lb in).