For 1990-2009 cars

### Removal Procedure

1. Remove the fuel fill pipe. Refer to Fuel Tank Filler Pipe Replacement.
2. Disconnect the fuel tank fill evaporative emission (EVAP) pipe quick connect fitting (1) at the fuel pump module. Refer to Plastic Collar Quick Connect Fitting Service.
3. Remove the fuel tank fill EVAP pipe.

### Installation Procedure

1. Install the fuel tank fill EVAP pipe.
2. Connect the fuel tank fill EVAP pipe quick connect fitting (1) to the fuel pump module. Refer to Plastic Collar Quick Connect Fitting Service.
3. Install the fuel fill pipe. Refer to Fuel Tank Filler Pipe Replacement.