For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Driver and Passenger Seat Replacement .
2. Remove the seat back recliner handle. Refer to Driver Seat and Passenger Seat Recliner Handle Replacement .
3. Remove the seat back recliner cover. Refer to Front Seat Back Recliner Outer Trim Panel Replacement .

1 | Seat Cushion Frame Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip Fold the seat back forward to access the bolts. Tighten
25 N·m (18 lb ft)

2 | Seat Outer Adjuster Assembly
3 | Seat Adjuster Handle Assembly

#### Procedure

1. Loosen the seat cushion frame bolts on the inner adjuster.
2. Install the seat adjuster spring and handle to the outer adjuster.
3. Loose install the outer adjuster to the seat cushion frame and align handle.
4. Use the handle to load the pressure onto the spring and into correct position.
5. Tighten the seat cushion frame bolts on the inner and outer adjuster.
6. Test the operation of the seat adjuster handle.

4 | Seat Adjuster Retaining Spring Tip Take note of the orientation of the spring for installation.