For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Position window approximately half way down.
2. Remove the interior trim panel. Refer to Door Trim Panel Replacement .
3. Remove the water deflector. Refer to Door Water Deflector Replacement .

1 | Front Side Door Window Regulator to Window Bolts (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Door Window Tip Adjust the door window. Refer to Door Window Adjustment .