For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .

1 | Air Inlet Grille Panel Screw (Qty: 6) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Air Inlet Grille Panel Retainer (Qty: 4)
3 | Air Inlet Grille Panel Assembly

#### Procedure

Upon installation of the air inlet grille panel to the windshield, secure the 3 upper clips on the grille panel to the bottom edge of the windshield, prior to securing the air inlet grille panel screws and retainers.