For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the folding top, position the No.1 bow in the upright position.

1 | Retainer Folding Top Cover No. 1 Bow Screw (Qty: 10) Notice: Refer to Fastener Notice in the Preface section. Tip The retainer is located on the front inside edge of the folding top. Tighten
2 N·m (18 lb in)

2 | Folding Top Cover No. 1 Bow Retainer