For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Stud | 10 N·m | 89 lb in
Air Conditioning (A/C) Condenser Bolt | 9 N·m | 80 lb in
Charge Air Cooler Pipe Bolt | 7 N·m | 62 lb in
Coolant Heater Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Exhaust Heat Shield Bolt | 23 N·m | 17 lb ft
Radiator Air Deflector Bolt | 9 N·m | 80 lb in
Radiator Bolt | 25 N·m | 18 lb ft
Radiator Surge Tank Bracket Nut | 9 N·m | 80 lb in
Radiator Upper Support Bracket Nut | 9 N·m | 80 lb in
Surge Tank Nut | 9 N·m | 80 lb in
Thermostat Housing Bolt | 10 N·m | 89 lb in
Thermostat Housing Cover Bolt | 10 N·m | 89 lb in
Turbocharger Coolant Feed Pipe Bracket | 10 N·m | 89 lb in
Turbocharger Coolant Feed Pipe Fitting | 35 N·m | 26 lb ft
Turbocharger Coolant Feed Pipe Bolt | 35 N·m | 26 lb ft
Turbocharger Coolant Return Pipe Bolt | 35 N·m | 26 lb ft
Water Pump Access Plate Bolt | 10 N·m | 89 lb in
Water Pump Bolt | 25 N·m | 18 lb ft
Water Pump Drain Plug | 22 N·m | 16 lb ft
Water Pump Sprocket Bolt | 10 N·m | 89 lb in