For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Side Door Trim Panel Screw, if equipped Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Inside Door Handle Bezel Plug
3 | Front Side Door Trim Panel Cover Assembly

#### Procedure

1. Remove the ashtray, if equipped.
2. Disconnect the electrical connectors.

4 | Front Side Door Trim Panel Screw (Qty: 3) Tighten 2 N·m (18 lb in)
5 | Front Side Door Trim Panel Assembly

#### Procedures

1. Use a J 38778 Door Trim Clip Remover to aid in the removal of the door trim panel.
2. Pull up on front side door lock retainer to disengage cable.
3. Disconnect electrical connectors.

#### Special Tools

J 38778 Door Trim Clip Remover

6 | Front Side Door Trim Retainer (Qty: 9)