For 1990-2009 cars

#### Limited Slip Differential Diagnosis

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you review the general description and perform the necessary inspections? | -- | Go to Step 2 | Go to Diagnostic Starting Point - Locking/Limited Slip Rear Axle
2 | Measure the rotational force of the axle using the following procedure:

1. Block the front wheels.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .
4. Using the J 28733-B Front/Rear Spindle Remover, measure the rotational force of the axle.
5. Repeat the procedure for the other axle.

Does the force measure outside the specified range?

22-271 N·m (30-200 lb ft)

Go to Step 3

System OK

3 | Repair the rear axle. Did you complete the repair? | -- | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | -- | Go to Step 2 | System OK