For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear bumper extension. Refer to Rear Bumper Extension Replacement .
2. Disconnect the electrical harness connector from the tab on the rear bumper valance center panel.
3. Remove the two lower backup lamp screws from the rear bumper valance center panel.

1 | Backup Lamp Assembly Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Backup Lamp Assembly Tip Replace or transfer the bulbs as needed.