For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
2. Remove the instrument panel compartment frame. Refer to Instrument Panel Compartment Door Opening Frame Replacement .
3. Remove the knee bolster assembly. Refer to Knee Bolster Replacement .

1 | Instrument Panel Lower Trim Panel Screw (Qty: 1) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Instrument Panel Lower Trim Panel Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the instrument lower trim panel, transfer all necessary components.

3 | Retainer Clips (Qty: 6)