For 1990-2009 cars

## Radio Rear Speaker Replacement Lock Pillar

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the lock pillar trim. Refer to Body Lock Pillar Trim Panel Replacement .

1 | Body Lock Pillar Garnish Molding Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Radio Rear Speaker Assembly

#### Procedure

If the speaker is heat staked in place, replace the body side front garnish molding. A new molding will include the speaker.

## Radio Rear Speaker Replacement Subwoofer

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear window panel trim. Refer to Rear Window Panel Trim Replacement .

1 | Radio Quarter Speaker Nut (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Radio Rear Speaker Assembly