For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Hood Strut Assembly Warning: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury. Caution: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.

Tip
Remove the metal clip at the ends of the assist rod, then pull away from stud.