For 1990-2009 cars

System | DTCs Required to Set System Status to YES
--- | ---
Catalyst Monitor If an I/M System Status indicator did NOT update to YES during the Inspection/Maintenance (I/M) System Check , review each indicator and reference this table to determine each DTC associated with the I/M System Status Indicator. Each DTC listed below has specific conditions that must be met for the diagnostic to run. Included in these conditions are additional DTCs which, if set, will inhibit these DTCs from running. Reviewing and operating the vehicle within the Conditions for Running for each DTC listed below will allow the I/M System Status Indicators to transition to YES.
Catalyst | DTC P0420
EVAP | DTC P0443, P0449, P0458, P0459, P0498, or P0499 DTC P0446 DTC P0451, P0452, or P0453 DTC P0455 DTC P0496
Oxygen Sensor | DTC P0130, P0131, P0132, P0133, P2195, P2196, P2231, or P2297 DTC P0137, P0138, P0139, P0140, P2232, P2270, or P2271
Oxygen Sensor Heater | DTC P0030, P0031, P0032, P0053, or P0135 DTC P0033, P0034, or P0035 DTC P0036, P0037, P0038, or P0141