For 1990-2009 cars

## Remote Control Door Lock Receiver Programming and Setup Without Accessory 2 Way Remote

If the remote control door lock receiver is replaced, the following setup procedure must be performed with the scan tool:

1. Install a scan tool.
2. Turn ON the ignition with the engine OFF.
3. Select Body.
4. Select Remote Control Door Lock Receiver (RCDLR).
5. Select Module Setup.
6. Select Setup New RCDLR.
7. Follow the scan tool instructions.
8. Remove scan tool and exit vehicle when setup is done.

### Replacing Keyless Entry Transmitters

If a keyless entry transmitter is replaced, the following procedure must be performed:

Keyless Entry Transmitter Programming--Refer to Transmitter Programming .