For 1990-2009 cars

#### Tools Required

J 45866 Input Shaft Seal Installer

### Removal Procedure

1. Remove the transmission input shaft bearing retainer. Refer to Transmission Input Shaft Bearing Retainer Replacement .
2. Using a hammer and a punch, remove the input shaft seal from the input shaft bearing retainer.

### Installation Procedure

1. Using the J 45866 and a hammer, install the input shaft seal into the input shaft bearing retainer.

• | The spring side of the seal goes toward the tool

• | Ensure the seal is installed square

• | The tool will install the seal to the correct depth

2. Install the transmission input shaft bearing retainer. Refer to Transmission Input Shaft Bearing Retainer Replacement .