For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the air inlet grille. Refer to Air Inlet Grille Panel Replacement.
3. Remove the A/C condenser tube assembly from the evaporator tube. Refer to Compressor Hose Assembly Replacement.

1 | A/C Evaporator Hose Assembly Nut Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | A/C Evaporator Hose Assembly Bolt Tighten 9 N·m (80 lb in)
3 | Sealing Washer (Qty: 2)

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement.

4 | A/C Evaporator Hose Assembly