For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Open the folding top and stowage compartment lid.

1 | Folding Top Pivot Bracket Nut (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tip

• | Lift only the side of the folding top that the pivot bracket is to be replaced high enough to clear the adjusting pin.

• | Mark location relative to body of bracket.

• | Leave the alignment pin loose. Loose fit the top latch. Latch top to header. Check seal fit to door glass prior to tightening top alignment pin.

• | Adjust the folding top. Refer to Folding Top Adjustment .

Tighten
9 N·m (80 lb ft)

2 | Folding Top Pivot Bracket