For 1990-2009 cars

### Removal Procedure

1. Remove the rear differential. Refer to Propeller Shaft, Differential, and Driveline Support Replacement .
2. Remove the 9 carrier cover bolts (6).
3. Using the pry tabs (4, 5, 7), remove the carrier cover (3) from the differential carrier (1).
4. Remove the O-ring seal (2) from the cover (3).

### Installation Procedure

1. Install the housing cover O-ring (2) into the groove on the housing cover (3).
2. Apply a light coat of oil to the housing cover O-ring (2) and install the housing cover (3) onto the housing (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the 9 side cover bolts (4).

Tighten
Tighten the 9 side cover bolts in a criss-cross pattern to 25 N·m (18 lb ft).

4. Install the rear differential. Refer to Propeller Shaft, Differential, and Driveline Support Replacement .