For 1990-2009 cars

1. Loosen the jam nut on the tie rod (2).
2. Rotate the inner tie rod (1) to the required toe specification setting. Refer to Wheel Alignment Specifications .

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the jam nut on the tie rod.

Tighten
Tighten the front tie rod jam nut to 68 N·m (50 lb ft).

4. Check the toe setting after tightening.
5. Adjust the toe setting if necessary.