For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the tail lamp assembly. Refer to Tail Lamp Replacement .
2. Remove the right and left rear wheelhouse. Refer to Rear Wheelhouse Panel Liner Replacement .

1 | Rear Fascia Retainers (Qty: 4)
2 | Rear Fascia Screws (Qty: 7) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Rear Fascia Bracket Screws (Qty: 8)

#### Procedure

Reach between the fascia and the quarter panel to loosen the bolts.

Tighten
2 N·m (18 lb in)

4 | Rear Fascia Bracket Push-Pin (Qty: 2)
5 | Rear Fascia Tip Disconnect the lamp connectors.