For 1990-2009 cars

1. Install two new friction washers.
2. Install the engine front cover with a new gasket.

Notice: Refer to Fastener Notice in the Preface section.

Important: The center bolt (1) should be tightened last.

3. Install the engine front cover bolts.

Tighten
Tighten the engine front cover bolts to 25 N·m (18 lb ft).

4. Install the long water pump bolt.

Tighten
Tighten the water pump bolt to 25 N·m (18 lb ft).

5. Install the accessory drive belt tensioner.
6. Install the accessory drive belt tensioner bolt.

Tighten
Tighten the bolt to 45 N·m (33 lb ft).