For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left instrument panel closeout/insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side .
2. Remove the left instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement .

1 | Knee Bolster Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Knee Bolster Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the knee bolster assembly, transfer all necessary components.

3 | Retainer Clips (Qty: 3)