For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement .

1 | Instrument Panel Cluster Assembly Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Cluster Assembly

#### Procedure

1. Disconnect the electrical connector.
2. When replacing the cluster, refer to Control Module References .