For 1990-2009 cars

Windshield wiper blades should be inspected for wear and cracking. See Scheduled Maintenance for more information.

Replacement blades come in different types and are removed in different ways. For proper type and length, see Maintenance Replacement Parts .

To replace the windshield wiper blade assembly:

1. Lift the wiper arm away from the windshield.
2. Push the release lever (B) to disengage the hook and push the wiper arm (A) out of the blade (C).
3. Push the new wiper blade securely on the wiper arm until you hear the release lever click into place.