For 1990-2009 cars

The following services should be performed at the first maintenance service (I or II) after the indicated miles (kilometers) shown for each item.

#### Additional Required Services

Service and Miles (Kilometers) | 25,000 (40 000) | 50,000 (80 000) | 75,000 (120 000) | 100,000 (160 000) | 125,000 (200 000) | 150,000 (240 000)
--- | --- | --- | --- | --- | --- | ---
Inspect fuel system for damage or leaks. | · | · | · | · | · | ·
Inspect exhaust system for loose or damaged components. | · | · | · | · | · | ·
Replace engine air cleaner filter. See Engine Air Cleaner/Filter . |  | · |  | · |  | ·
Replace spark plugs. An Emission Control Service. |  |  |  | · |  |
Engine cooling system service (or every five years, whichever occurs first). An Emission Control Service. See footnote (i). |  |  |  |  |  | ·
Inspect engine accessory drive belt. An Emission Control Service. See footnote (g). |  |  |  |  |  | ·