For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the engine sight shield. Refer to Engine Sight Shield Replacement.
2. Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Engine Appearance Cover

#### Procedure

Disconnect the electrical connector

2 | Engine Appearance Cover Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use a new gasket.

Tighten
20 N·m (15 lb ft)