For 1990-2009 cars

#### Special Tools

EN-44887 Oil Filter Wrench

For equivalent regional tools, refer to Special Tools.

1. Install a new oil filter (2) on the oil filter cap (1).
2. Lubricate the oil filter cap O-ring with 5W30 engine oil.

Caution: Refer to Fastener Caution in the Preface section.

3. Use the EN-44887 wrench to install the oil filter and cap. Tighten the oil filter and cap to 22 N·m (16 lb ft).